D12V8 FPC Specifications

A computer generated image of a lizard

AI-generated content may be incorrect.

PCB Type : Flexible PCB

Board type : Single pieces

Layer : 2 Layers

Material : Polyimide Flex:

FPC Thickness : 0.13 mm

Solder Mask (Coverlay) : Black Coverlay

Silkscreen : White / Black

Stiffener : BOT FR4 : 0.15 mm

filename: *Main-B\_Stiffener.gbr*

Surface Finish : Immersion gold (ENIG) (1U")

Finished Copper : 0.5 oz **Annealed** Cu (18μm)

E-test : 100%

3M/Tesa tape : BOT

Glue: *Main-B\_3M\_Adhesive.gbr*

Backing Tape: *Main-B\_3M\_Backing.gbr*

SMT: TOP