PCB Type:FR-4

Board type:2pieces/1 Board

Layer:2 Layers

PCB Thickness:1.6mm

Solder Mask:Green

Silkscreen:White

Surface Finish:Immersion gold(1u)

Finished Copper:1.0oz

E-test:100%

SMT:Top&Bottom